|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Site / Area:** | |  | | **Date of assessment:** |  | **Risk Assessment #:** | **064RA** |
| **Completed by (name):** | |  | | **Signature:** |  | | |
| **In Consultation with** | |  | | **Signature:** |  | | |
| **Identify / describe activity, equipment, area or event you are assessing:** | | | | | **OXY-ACETYLENE WELDING KIT** | | |
| **In conjunction with this risk assessment, training / education and development of a relevant SOP may be required.** | | | | | | | |
| **Step 1:** **Identify the hazard/s:**What do you believe are the hazards?(Refer Risk Assessment Guideline (015G)) | | **Step 2: Assess the risks:**  What do you believe are the risks?  (Refer *Risk Assessment Guideline (015G)*) | | **Step 3: Reducing the risk:** What do you believe can be done to reduce the risk? (Refer *Risk Assessment Guideline (015G)*) | | |
| **What could cause harm?** | | **What could go wrong?** | | **Controls** | | |
| **Hazardous Manual tasks**   * Manual Handling of the plant and gas bottles | | * Pushing/pulling the oxy-acetylene set around the workshop * Moving projects on/off the bench | | * Plant is mounted on a trolley for ease of movement * All workers are trained in safe manual handling techniques | | |
| **Hazardous Chemicals**   * Storage of gas bottles | | * Sprains / strains * Gas leak | | * Gas bottles must be secured to trolley &/or wall at all times. * Store cylinders in an upright position to ensure the safety device functions correctly * When cylinders not in use, cylinder valve to be kept closed. | | |
| **Radiation**   * Welding Flash | | * Damage to eyes * Burns | | * Welding mask with correct grade lens must be worn * Where practical suitable partitions to be placed around work area * Safety glasses to be worn * Other persons inside work area must wear similar eye protection Install non-flammable screens and partitions. * Signs used to warn that welding is occurring. * Provide PPE including filter shades for goggles and face shields to protect the eyes from radiation. Gloves and other protective clothing to be worn to cover exposed skin. | | |
| **Airborne Contaminants**   * Noxious fumes or flames | | * Burns * Respiratory problems * death | | * Gloves to be worn to prevent burns to hands and lower arm * Mechanical extraction fitted where possible * Use in well ventilated areas * Long sleeve clothing to be worn, secured. * Welding apron with correct grade protection to be worn * Welded material to be allowed to cool down before handling * Any other work participants to follow same requirements * Operator to ensure that work pieces are to be free of any oils or other flammable materials before welding occurs. * No flammable materials or liquids to be near the welding area * Gas hoses to be checked for any damage before starting welding * DO NOT USE IF ANY SUSPICIOUS DAMAGE IS EVIDENT * ENSURE FLINT LIGHTER IS READY TO USE BEFORE TURNING ON GAS * TURN ON ACETYLENE GAS FIRST AND LIGHT IT BEFORE TURNING OXYGEN ON (Refer to operating instructions) * Gas hoses to be well clear of weld splatter at all times * Ensure welding area is well ventilated * Operator to be aware of proximity of a fire extinguisher * ENSURE WELD TORCH VALVES AND GAS REGULATORS ARE CORRECTLY CLOSED WHEN WELDING/CUTTING COMPLETED * Flashback arresters are fitted to the hand-piece. | | |
| **Machinery & Equipment**   * Fire & explosion | | * Serious injuries * Burns | | * Work areas are well ventilated * Work area is free from rubbish, paper or dust that could be potential fuel sources or produce dust explosions. * Use flash back arrestors on gas hoses to prevent the flames travelling back and igniting the gas in cylinder. * Drain and purge equipment, such as gas hoses, and lock the gas off at the valve immediately after use. * Do not store flammable and combustible materials near welding area. * Fire fighting equipment readily accessible near welding area. | | |
| **Gravity**   * Slips, trips and falls | | * Sprains / strains | | * Ground in work area to be free of obstructions * Ground to be checked for any grease or liquid spills * Safety footwear to be worn and care taken to prevent slips and trips * Work area to be clear of any obstructions which will might cause interruptions to welding operation * Any other work participants to follow same requirements * Hoses to be kept secure and clear of working zones. | | |
| **Extreme Temperatures**   * Prolonged working with heat | | * Dehydration * Heat strain | | Take regular breaksCool potable water available | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Authorised by:** |  | **Signature:** |  | **Date:** |  |

**Review hazard/risk assessment if task or circumstances change and at intervals appropriate to the level of risk (minimum 5 years).**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Step 4: Monitor & review:**  (Refer to hazard sheet)  **Please tick Yes or No** | | | | | | | | |
| **Were the controls effective?** | | | | **Were there any unforeseen hazards/ incidents?** | | | | **New controls** |
| **Yes** |  | **No** |  | **Yes** |  | **No** |  |
| **DETAILS** | | | | **DETAILS** | | | | **DETAILS** |
|  | | | |  | | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name:** |  | **Signature:** |  | **Date:** |  |